;This file is used to provide xscan with special case information needed to work porperly with
;certain scanners.  This file is currently checked only when a scanner is accessed via a TWAIN
;data source


;THIS IS HINT FILE VERSION 5.5

[Info]

<END>

[Default]
<END>

;WIA scanner hint

[Visioneer OneTouch 8600 USB]
WIADEVICETYPE=SCANNER
WIAMAXWIDTH=8.503937
WIAMAXHEIGHT=11.692913
WIAUI=HIDE
<END>

[UMAX Astra 2200(USB)]
WIAADF=NO
WIADOUBLEBUFFER=FALSE
WIAXFERMECH=NATIVE
WIAMAXWIDTH=8.503937
WIAMAXHEIGHT=11.692913
WIAUI=HIDE
<END>

;TWAIN scanner hints

;HP ScanJet 5300C
;HP ScanJet 5300Cse
[HP PrecisionScan 3.02 Rev 1.0]
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
RESRANGE=50,600,50
TWAINUI=HIDE
<END>

;HP ScanJet 5300C
[HP PrecisionScan 3]
RESRANGE=100,600,50
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
TWAINUI=HIDE
<END>

;HP ScanJet 6450C WIA WinME
[WIA-Hewlett-Packard ScanJet 6300C Rev 1.0]
TWAINUI=SHOW
<END>

;HP ScanJet 6250
[WIA-Hewlett-Packard ScanJet 5200C Rev 1.0]
TWAINUI=SHOW
<END>

;Microtek ScanMaker 3600 per Flora, running UI down it truncates sizes to whole inches
[Microtek ScanWizard 5 Rev 5]
TWAINUI=SHOW
<END>

;Syscan (hinted UI up because they need to do a calibration step or the image won't look good)
[TravelScan V1.2 Rev 3]
TWAINUI=SHOW
ADF=SHEET
MAXHEIGHT=14
<END>

;Primax Colorado USB 19200
;Primax Colorado 1200P in win 95,98.
[PRIMAX Power TWAIN Rev 1.0]
BUFFERSIZE=PREFERRED
MAXHEIGHT=11.7
TWAINUI=SHOW
<END>

;Primax Colorado 1200P in Win NT.
[Colorado 600p/1200p Rev 2.0]
BUFFERSIZE=PREFERRED
TWOPASS=DISABLED
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[Vivitar ViviScan Compact II]
ADF=NO
RESRANGE=100,400,100
MAXWIDTH=8.503937
MAXHEIGHT=11.69
TWAINUI=HIDE
<END>

[KODAK DC200/DC210 Zoom Acquire Rev 1.0]
ADF=CAMERA
INVERTC=YES
TWAINUI=SHOW
<END>

;Epson Perfection 636U
[EPSON TWAIN 3(32-bit) Rev 3.1]
INDICATORS=ON
TWAINUI=HIDE
<END>

[EPSON TWAIN 3(32-bit) Rev 3]
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=SHOW
<END>

[MagicScan32 V3.1 Rev 3]
TWOPASS=DISABLED
ENDDELAY=10
MAXWIDTH=8.5
MAXHEIGHT=12
CONTRASTRANGE=-999,0,-499
TWAINUI=HIDE
<END>

[Storm PageScan USB Rev 2]
PAGESIZE=AUTOMATIC
ADF=SHEET
CONTRASTRANGE=-999,999,0
TWAINUI=HIDE
<END>

[DRSCAN30EPP Rev 1]
TWOPASS=DISABLED
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
RESRANGE=50,400,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[DRSCAN30HREPP Rev 1]
RESRANGE=50,400,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>


[ImageReader LE v1.3.2 Rev 1.0]
TWOPASS=DISABLED
REGFLAT=CENTER
TWAINUI=HIDE
<END>

[ScanExpress 12000P]
TWOPASS=DISABLED
RESRANGE=100,1200,50
ADF=NO
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[6120P/32 V4.04 Rev 1.6]
ADF=NO
MAXWIDTH=8.50
MAXHEIGHT=11.69
INVERTB=YES
TWAINUI=HIDE
<END>

[WidowVIEW-32S 2.67 English Rev 2.67]
THRESHOLD=LOWLIGHT		
DFLTBRIGHT=USE MSG_SET	
BRIGHTRANGE=0,500,250
CONTRASTRANGE=0,500,250
RESRANGE=50,600,25
ADF=NO
MAXWIDTH=8.5
MAXHEIGHT=11.69
INVERTC=YES
INVERTG=YES
TWAINUI=SHOW
<END>

;Genius-Kye Color Page Vivid Pro USB 
[ColorPage-Vivid Pro USB Rev 2]
UI=BEHIND
XFERMECH=NATIVE
TWAINUI=HIDE
<END>

[ColorPage-View Rev 1]
TWOPASS=DISABLED
REGFLAT=CENTER
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[TotalScan Express Rev 1.0]
RESRANGE=100,400,50
TWAINUI=HIDE
<END>

[HP LaserJet 1100 Series Rev 1.0]
RESRANGE=100,400,50
BUFFERSIZE=MINMAX
ADF=SHEET
MAXWIDTH=8.503937
MAXHEIGHT=11.023622
TWAINUI=SHOW
<END>

[HP OfficeJet Series 600]
ENDDELAY=25
TWAINUI=SHOW
<END>

[HP OfficeJet Series 700]
TWAINUI=SHOW
<END>

;Mustek Plug-N-Scan 1200CU (USB)
[Mustek 1200 CU Rev]
RESRANGE=100,400,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

;Mustek Plug-n-Scan 1200ED (Parallel)
[Mustek 1200 ED Rev]
ADF=NO
RESRANGE=100,400,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[Mustek 1200 LS Rev 1.0]
RESRANGE=50,400,50
BRIGHTRANGE=-127,127,2
CONTRASTRANGE=-127,127,0
DFLTCONTRAST=USE MSG_SET
DFLTBRIGHT=USE MSG_SET
TWAINUI=HIDE
<END>

[HP ScanJet 5s Rev 1.0]
RESRANGE=50,400,50
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
TWAINUI=SHOW
<END>

[ESCAN_32 600 v1.00 Rev 1.0]
RESRANGE=50,400,50
MAXWIDTH=8.5
MAXHEIGHT=11
TWAINUI=SHOW
<END>

[Dexxa Flatbed Scanner 4800 Rev 1.0]
RESRANGE=50,400,50
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=11
UI=BEHIND
TWAINUI=SHOW
<END>

[FUJITSU TWAIN32(M3091DC) Rev 1.0]
REGADF=CENTER
TWAINUI=HIDE
<END>

;Fujitsu ScanPartner 93GX
[Fujitsu Limited TWAIN Driver Rev 7.2]
MAXWIDTH=8.503937
MAXHEIGHT=14.015748
CHECKFEEDERENABLED=YES
COLORBITDEPTH24=YES
TWAINUI=HIDE
<END>

[EasyPhoto ImageWave Rev 1.2]
RESRANGE=200,300,100
UI=BEHIND
MAXWIDTH=8.5
MAXHEIGHT=11.69
TWAINUI=HIDE
<END>

[Xerox WorkCentre 480cx Rev 4.0]
[Xerox WorkCentre 385 Rev 3.1]
;These are the hints for the Xerox WorkCentre 480CX
;The driver name will need to be renamed when they have a final version of
the driver
DFLTCONTRAST=USE MSG_SET
RESRANGE=100,400,100
ADF=SHEET
TWAINUI=HIDE
<END>

[CanoScan N650U/N656U Rev 5.7]
MAXWIDTH=8.5
MAXHEIGHT=11.69
THRESHOLD=LOWLIGHT
TWAINUI=HIDE
IGNORECANCEL=ONEBUF
<END>

[CanoScan FB630U/FB636U Rev 5.3]
TWAINUI=HIDE
<END>

[CanoScan FB320P/FB620P Rev 3.0]
ADF=NO
TWAINUI=HIDE
THRESHOLD=LOWLIGHT
<END>

[ARTEC AM12E Plus]
RESRANGE=50,400,50
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
MAXWIDTH=8.500000
MAXHEIGHT=11.700000
TWAINUI=HIDE
<END>

[Easy Twain Module 32(Epp Mode)]
RESRANGE=50,600,50
BRIGHTRANGE=-100,100,-93
CONTRASTRANGE=-90,1,1
INVERTB=YES
ADF=NO
GETBRIGHTNESS=BADCAP
GETCONTRAST=BADCAP
GETRES=BADCAP
MAXWIDTH=8.464567
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[EasyPhoto SmartPage]
UI=BEHIND
RESRANGE=75,600,25
TWAINUI=SHOW
<END>

[4830P (32-Bit TWAIN Source) Rev 4.0]
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

;UMAX 1200S DS installed from Win 98SE CD
[UMAX TWAIN DS Rev 2.38]
INVERTC=YES
INVERTB=YES
INVERTG=YES
MAXWIDTH=8.503937
MAXHEIGHT=14.015748
TWAINUI=HIDE
<END>

;UMAX 3400
;UMAX Astra 2200u
[VistaScan32 V3.75 Rev 3.1]
BRIGHTRANGE=0,1000,500
CONTRASTRANGE=-999,-499,0
;ENDDELAY=20
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

;UMAX Astra 4000U
;   4000U is a legal size scanner, need to run wizard to select legal size
;UMAX Astra 2000P
;UMAX Astra 2000U
;UMAX Astra 2100U
;UMAX Astra 2200
[VistaScan32 V3.52 Rev 3.1]
[VistaScan32 V3.51 Rev 3.1]
[VistaScan32 V3.5]
CONTRASTRANGE=-999,0,-499
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
;ENDDELAY=20
TWAINUI=HIDE
IGNORECANCEL=YES
<END>

[VistaScan32 V2.40]
[VistaScan32 V2.40 Rev 2.3]
TWAINUI=HIDE
FCW=YES
<END>

[VistaScan32 V2.43]
[VistaScan32 V2.43 Rev 2.4]
;if your scanner has an automatic document feeder, delete or comment (;)
;the line ADF=NO and add a line TWOPASS=DISABLED in this section
;If you are using the Umax 1200S, delete the (;) in front of the ENDDELAY = 20
;ENDDELAY=20
ADF=NO
TWAINUI=HIDE
FCW=YES
<END>

;UMAX Astra 6400
[VistaScan32 V3.72 Rev 3.1]
XFERMECH=NATIVE
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=SHOW
<END>

;HP ScanJet 5370C
;NOTE, the Rev 1.0 version of this driver is slow
;  due to the fact that it creates a log file
;  with several entries for each TWAIN call in it
[HP PrecisionScan Pro 2.5 Rev 1.0]
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[HP OfficeJet R PrecisionScan Rev 1]
ADF=YES
RESRANGE=100,600,50
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
TWOPASS=DISABLED
PAGESIZE=AUTOMATIC
UI=BEHIND
TWAINUI=HIDE
<END>

[HP PrecisionScan 1.01]
RESRANGE=50,400,50
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
PAGESIZE=AUTOMATIC
WNTTHREADPRIORITY=LOW
UI=BEHIND
TWAINUI=HIDE
<END>

[HP PrecisionScan 1.0 Rev 1.0]
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
TWAINUI=SHOW
RESRANGE=100,600,50
<END>

[HP PrecisionScan Pro 1.0]
BRIGHTRANGE=-1000,1000,1
CONTRASTRANGE=-1000,1000,1
RESRANGE=100,600,50
MAXHEIGHT=14.02
TWOPASS=DISABLED
TWAINUI=HIDE
XFERCOUNT=1
UI=BEHIND
<END>

;HP Scanjet 4100C (USB)
[HP PrecisionScan LT 1.0 Rev 1]
[HP PrecisionScan LT 1] 
ADF=NO	
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
RESRANGE=100,400,50
UI=BEHIND
PAGESIZE=AUTOMATIC
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

;HP ScanJet 4200C (Rev 1.0)
;HP ScanJet 3200C (Rev 1.0)
[HP PrecisionScan LT 2.0 Rev]
ADF=NO	
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
RESRANGE=100,400,50
UI=BEHIND
PAGESIZE=AUTOMATIC
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

;HP ScanJet 3300C (USB)
[HP PrecisionScan LT 3.0 Rev 1.0]
ADF=NO	
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
RESRANGE=100,400,50
UI=BEHIND
PAGESIZE=AUTOMATIC
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

;HP Scanjet 6250C (SCSI/USB)
[HP PrecisionScan 2.0]
;HP Scanject 5200Cse
;HP Scanject 5200C
[HP PrecisionScan 2.0 Rev 1.0]
RESRANGE=100,400,50
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
TWAINUI=SHOW
<END>

;HP ScanJet 6250c (SCSI/USB) and possibly others, OEM driver installed by windows 2000)
[HP ScanJet Source Rev 1.0]
RESRANGE=100,400,50
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
MAXWIDTH=8.503937
MAXHEIGHT=14.015748
GRAY4=NO
UI=BEHIND
TWAINUI=SHOW
<END>

;HP ScanJet 6350C (SCSI/USB)
[HP PrecisionScan Pro 2.0 Rev 1.0]
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
MAXWIDTH=8.503937
MAXHEIGHT=14.015748
UI=BEHIND
TWAINUI=HIDE
<END>

[HP PhotoSmart Photo Scanner Rev 1.0]
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
MAXHEIGHT=7.0
MAXWIDTH=5.0
RESRANGE=100,2400,50
ADF=CAMERA
TWAINUI=SHOW
<END>

[600P (32-Bit TWAIN Source) Rev 4]
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

[Microtek ScanWizard (32bit) Rev 2.5]
[Microtek ScanWizard Rev 2.5]
[Microtek ScanWizard (32bit) Rev 2.4]
[Microtek ScanWizard Rev 2.4]
;if you have an E3 Plus or SlimScan C6, remove the (;) from the line below
;TWOPASS=DISABLED
;if you have a SlimScan C6, also remove the (;) from the line below
;MAXHEIGHT = 11.692913
;if you have a SlimScan C3, remove the (;) from the line below
;ENDDELAY=15
THRESHOLD=LOWLIGHT
RESRANGE=100,400,100
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
TWAINUI=HIDE
<END>

[600 III EP]
[600 III EP Plus]
RESRANGE=100,400,50
TWAINUI=HIDE
DFLTBRIGHT=USE MSG_SET
MAXHEIGHT=11.7
<END>

[Mustek 1200 III EP Rev 1]
TWAINUI=HIDE
SCANAREA=GETRECT
<END>

[Mustek 1200 III SP]
ADF=NO
MAXWIDTH=8.5
MAXHEIGHT=11.7
RESRANGE=100,400,100
DFLTBRIGHT=USE MSG_SET
BRIGHTRANGE=-127,127,1
DFLTCONTRAST=USE MSG_SET
CONTRASTRANGE=-127,127,1
TWAINUI=HIDE
<END>

[FlatbedScanner Rev 1]
DFLTBRIGHTVAL=63
BUFFERSIZE=MINMAX
TWOPASS=DISABLED
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

[WidowVIEW-32S]
INVERTC=YES
INVERTG=YES
BUFFERSIZE=MINMAX
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
RESRANGE=150,900,150
MAXWIDTH=11.535433
MAXHEIGHT=16.535433
TWAINUI=SHOW
<END>

[WidowVIEW Rev 2.6]
INVERTC=YES
INVERTG=YES
TWAINUI=SHOW
<END>

[Adara AdaraScan Rev 2.4]
TWAINUI=SHOW
BUFFERSIZE=PREFERRED
TWOPASS=DISABLED
<END>

[Perfection 600 (32 Bit) Rev 3.7]
MAXWIDTH=8.5
MAXHEIGHT=14
RESRANGE =100,400,100
BRIGHTRANGE=-100,100,0
CONTRASTRANGE=-100,100,0
ADF=NO
TWAINUI=SHOW
<END>

[Perfection 600 (32 Bit) Rev 3.53]
MAXWIDTH=8.5
MAXHEIGHT=14
RESRANGE=25,2400,25
TWAINUI=SHOW
<END>

[Perfection 600 (32) rev 3.5]
INVERTB=YES
INVERTC=YES
INVERTG=YES
TWAINUI=SHOW
<END>

[Info driver (32-BIT TWAIN Source)]
TWAINUI=SHOW
TWOPASS=DISABLED
BUFFERSIZE=PREFERRED
<END>

[Easy twain module rev 1.0]
INVERTC=YES
INVERTG=YES
TWAINUI=SHOW
<END>

[Brother MFL Pro Scanner Rev 1.0]
[Brother driver (32-BIT TWAIN Source)]
TWAINUI=SHOW
TWOPASS=DISABLED
BUFFERSIZE=PREFERRED
<END>

[Paragon PowerPro Rev 1.4]
REGFLAT=CENTER
BRIGHTRANGE=5,995,500
TWOPASS=DISABLED
ADF=NO
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[HP OfficeJet Pro PictureScan Rev 2.0]
RESRANGE=75,400,25
BUFFERSIZE=PREFERRED
MAXWIDTH=8.5
MAXHEIGHT=11
TWOPASS=DISABLED
TWAINUI=SHOW
<END>

[ColorFactory 2.0 Rev 1.0]
ENDDELAY=20
ADF=NO
TWAINUI=HIDE
<END>

[Nikon Scan 32 Rev 5.3]
ADF=NO
TWAINUI=SHOW
<END>

[Canon IS Scan Rev 1.1]
MAXWIDTH=8.51
MAXHEIGHT=14
ADF=SHEET
BUFFERSIZE=PREFERRED
TWAINUI=HIDE
<END>

[MyScan32 V1.2a Rev 3.1]
MAXWIDTH=8.5
MAXHEIGHT=11.7
ADF=SHEET
TWAINUI=HIDE
<END>

[Olympus Digital Vision]
TWAINUI=SHOW
<END>

[OLYMPUS C-2.1TE]
DFLTRES=100
ADF=NO
TWAINUI=SHOW
<END>

[EPSON PhotoPC 600]
TWAINUI=SHOW
<END>

[EPSON TWAIN(32-bit)]
ADF=NO
;MODEL: EPSON ES1000C (GT8500) 
;VERSION: 32-bit TWAIN 2.62
;5/4/98 sjl
;Pagis 2.0 
DFLTCONTRAST=USE MSG_SET
TWAINUI=HIDE
<END>

[CyberView]
[CyberView-32]
TWAINUI=SHOW
INVERTC=YES
INVERTG=YES
<END>

[WorkCentre 400c Series]
SCANNERID=WorkCentre 400c Series
TWAINUI=HIDE
<END>

[AV260C/32 V4]
BRIGHTRANGE=-127,127,0
MAXHEIGHT=11.7
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

[CanoScan 300]
[CanoScan 600]
RESRANGE=100,400,100
MAXHEIGHT=11.69
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

[Canon PowerShot 350]
TWAINUI=SHOW
<END>

[TotalScan Express Rev 1.0]
RESRANGE=100,400,100
MAXWIDTH=8.5
MAXHEIGHT=11.7
TWAINUI=HIDE
<END>

[Storm TotalScan]
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

[ViewStation AS6E v1]
BRIGHTRANGE=-100,100,0
TWAINUI=HIDE
<END>

[CT-F300E Flat Bed]
RESRANGE=75,400,25
BRIGHTRANGE=-1000,1000,0
MAXHEIGHT=11.69
MAXWIDTH=8.5
TWOPASS=DISABLED
XFERMECH=NATIVE
TWAINUI=HIDE
<END>

[Primax Colorado Direct / D600]
BUFFERSIZE=PREFERRED
ENDDELAY=15
TWAINUI=HIDE
<END>

[ScanMagic 4800P]
BRIGHTRANGE=-1000,1000,0
TWOPASS=DISABLED
MAXHEIGHT=11
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

;AcerScan Prisa 640U
[MiraScan V3.40 Rev 3.0]
;AcerScan 620U
;AcerScan Prisa 320P
[MiraScan V3.04 Rev 3.0]
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

;AcerScan Prisa 620PT
[MiraScan V3.01 Rev 3.0]
RESRANGE=100,300,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[MiraScan32 2.2]
[MiraScan32 V2.3]
BRIGHTRANGE=-127,127,0
BUFFERSIZE=PREFERRED
RESRANGE=75,300,25
MAXHEIGHT=11.69
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

[Imager 730/32 V4]
BRIGHTRANGE=-127,127,0
MAXHEIGHT=11.69
MAXWIDTH=8.5
TWAINUI=HIDE
<END>

[PaperPort OneTouch]
MAXWIDTH=8.5
MAXHEIGHT=11.69
TWAINUI=HIDE
<END>

[Visioneer OneTouch 8100 Rev 2.0]
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

; Visioneer OneTouch 7600 USB
[Visioneer OneTouch 7600 USB Rev 1.10]
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

;Visioneer OneTouch 5300 USB
[Visioneer OneTouch 5300 USB Rev 1.10]
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[Visioneer PaperPort 3]
[Visioneer PaperPort 6]
BRIGHTRANGE=-127,127,0
MAXHEIGHT=11.7
MAXWIDTH=8.5
RESRANGE=100,600,50
DFLTBRIGHT=USE MSG_SET
ADF=NO
PIXELTYPE=VANILLA
TWOPASS=DISABLED
BUFFERSIZE=PREFERRED
TWAINUI=HIDE
<END>

[FotoSnap 32]
TWAINUI=SHOW
<END>

;AGFA 1212p,1212U,1236s
[ScanWise 1.2 Rev 1]
INDICATORS=ON
RESRANGE=100,400,100
ADF=NO
BUFFERSIZE=MINMAX
PENDINGXFERS=YES
TWOPASS=DISABLED
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>


;Agfa Scanners
[FotoLook 32]
[FotoLook 32 V2]
[FotoLook 32 V3.00.05 - TWAIN Rev 1.0]
MAXHEIGHT=11.7
MAXWIDTH=8.5
BRIGHTRANGE=-1000,1000,0
CONTRASTRANGE=-1000,1000,0
BUFFERSIZE=PREFERRED
TWAINUI=HIDE
<END>

[FotoLook 32 V3]
BRIGHTRANGE=-999,999,0
CONTRASTRANGE=-999,999,0
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[ImageReader Ultra/32 V4]
MAXHEIGHT=11.7
MAXWIDTH=8.5
BRIGHTRANGE=-127,127,0
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
TWAINUI=HIDE
<END>

[Logitech PageScan USB]
PAGESIZE=AUTOMATIC
ADF=SHEET
TWAINUI=HIDE
<END>

[Logitech FreeScan]
[Logitech PageScan Scanner Rev 2]
[Xerox Document HomeCentre Rev 2]
BRIGHTRANGE=-1000,1000,0
[Logitech PageScan]
ADF=SHEET
INDICATORS=ON
PAGESIZE=AUTOMATIC
SCANNERID=Logitech PageScan Color
TWAINUI=HIDE
<END>

[VistaScan32 2.37]
TWOPASS=DISABLED
FCW=YES
TWAINUI=HIDE
<END>

[VistaScan32 V2.3]
RESRANGE=100,300,100
MAXHEIGHT=11.7
MAXWIDTH=8.5
TWOPASS=DISABLED
DFLTBRIGHT=USE MSG_SET
FCW=YES
TWAINUI=HIDE
<END>

[VistaScan32 V2.4]
MAXHEIGHT=11.7
MAXWIDTH=8.5
DFLTBRIGHT=USE MSG_SET
TWOPASS=DISABLED
FCW=YES
TWAINUI=HIDE
<END>

[VistaScan32 V3.1]
[VistaScan32 V3.1 Rev 3.1]
;if you have an Astra 1220S or 2400S, remove the (;) from the line below
;ENDDELAY=20
RESRANGE=50,600,50
CONTRASTRANGE=500,500,500
TWAINUI=HIDE
FCW=YES
<END>

[HP PictureScan 3.0]
[HP PictureScan 2.0]
UI=BEHIND
TWOPASS=DISABLED
INDICATORS=ON
TWAINUI=HIDE
<END>

[DeskScan II 2.9]
RESRANGE=50,400,50
WNTTHREADPRIORITY=LOW
TWAINUI=SHOW
<END>

[DeskScan II 2.8]
TWOPASS=DISABLED
[DeskScan]
WNTTHREADPRIORITY=LOW
UI=BEHIND
TWAINUI=HIDE
<END>

[HP OfficeJet Pro PictureScan]
RESRANGE=75,300,1
RESAPPRX=75,100,150,200,300,400,600
TWAINUI=HIDE
<END>

;Microtek Scanmaker X6 (USB)
;Microtek Slimscan C6 (USB)
[Microtek ScanWizard for USB Rev 1.3]
RESRANGE=100,400,50
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>


[Microtek 32-bit PageIn]
[Microtek 16-bit PageIn]
ADF=SHEET
REGADF=CENTER
TWAINUI=HIDE
<END>

[Microtek ScanWizard (32bit) Rev 2.30]
[Microtek ScanWizard (32bit) Rev 2.31]
[Microtek ScanWizard (32bit) Rev 2.32]
[Microtek ScanWizard Rev 2.30]
[Microtek ScanWizard Rev 2.31]
[Microtek ScanWizard Rev 2.32]
INVERTG=YES
INVERTC=YES
[Microtek ScanWizard (32bit) Rev 2]
RESRANGE=100,400,100
[Microtek ScanWizard (32bit)]
[Microtek ScanWizard]
;If your Microtek scanner does have an ADF attached, remove or comment (;) the line below
ADF=NO
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
RESAPPRX=75,100,150,200,300,400,600
TWAINUI=HIDE
<END>

[PSDScan]
ADF=SHEET
REGADF=CENTER
TWAINUI=HIDE
<END>

[UMAX ScanIt/32  V3.2]
;UMAX Astra 300p, UMAX ScanIt/32 V3.20, Pagis 2.0, TJP 5/5/98
;Note that the 3.30 rev of the ScanIt driver has to run Native mode transfer
INVERTB=YES
TWOPASS=DISABLED
ADF=NO
CONTRASTRANGE=-128,128,0
BRIGHTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=11
XFERMECH=NATIVE
TWAINUI=HIDE
<END>

[UMAX ScanIt/32  V3.3]
;UMAX Astra 300p, UMAX ScanIt/32 V3.30, Pagis 2.0, TJP 5/5/98
;Note that the 3.30 rev of the ScanIt driver has to run UI up.
INVERTB=YES
TWOPASS=DISABLED
ADF=NO
CONTRASTRANGE=-128,128,0
BRIGHTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=11
TWAINUI=SHOW
<END>

[UMAX PageOffice Color]
ADF=SHEET
REGADF=CENTER
TWAINUI=HIDE
<END>

[EPSON Scanners]
;If your Epson scanner does have an ADF attached, remove or comment (;) the line below
BRIGHTRANGE=-3,3,0
ADF=NO
TWAINUI=HIDE
<END>

[Mustek F/B Scanner]
[Mustek F/B Scanner (EPP)]
[F/B Scanner (EPP-II)]
UI=BEHIND
BUFFERSIZE=MINMAX
RESRANGE=100,600,100
CONTRASTRANGE=-128,128,0
BRIGHTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=11.69
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
ENDDELAY=20
;If your Mustek scanner does have an ADF attached, remove or comment (;
ADF=NO
TWAINUI=HIDE
<END>

[Paragon Page Color]
ADF=SHEET
REGADF=CENTER
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
BRIGHTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=14
TWAINUI=HIDE
<END>

[4830P (32-Bit TWAIN Source)]
[9630P (32-Bit TWAIN Source)]
TWOPASS=DISABLED
BUFFERSIZE=PREFERRED
TWAINUI=HIDE
<END>

[600P (32-Bit TWAIN Source)]
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

[OpticPro A3I]
TWOPASS=DISABLED
TWAINUI=HIDE
<END>

; Plustek Flatbed
[Flatbed Scanner (32-bit) Rev 3]
TWOPASS=DISABLED
BUFFERSIZE=PREFERRED
ADF=NO
TWAINUI=HIDE
<END>

;Plustek 9636T
[Flatbed Scanner]
RESRANGE=75,600,25
ENDDELAY=10
TWOPASS=DISABLED
REGFLAT=CENTER
TWAINUI=HIDE
<END>

;IBM Ideascan P
[IBM Scanner (011) Rev 2.35]
REGFLAT=CENTER
MAXWIDTH=8.503937
MAXHEIGHT=11.692913
TWAINUI=HIDE
<END>

[IBM Flatbed Scanner-32]
REGFLAT=CENTER
TWOPASS=DISABLED
SCANNERID=WorkCentre 400c Series
TWAINUI=HIDE
<END>

;IBM ADF Color Scanner
; Plustek Spectra 1200
[Sheetfed Scanner (32) Rev 3]
BUFFERSIZE=PREFERRED
ADF=SHEET
TWAINUI=HIDE
<END>

[DynaScan_32 V3]
ENDDELAY=15
TWAINUI=HIDE
<END>

[AV360C/16 Scanner V3]
INVERTB=YES
ADF=NO
TWAINUI=HIDE
<END>

[ColorTake Scan 6630-32]
RESRANGE=50,1200,50
ADF=SHEET
TWAINUI=HIDE
<END>

[MrScan/32-Expert V3]
INVERTB=YES
TWAINUI=HIDE
<END>

[MultiPASS Source]
ADF=SHEET
UI=BEHIND
CONTRASTRANGE=-128,128,0
BRIGHTRANGE=-1000,1000,0
MAXWIDTH=8.5
MAXHEIGHT=11
TWAINUI=SHOW
<END>

[MultiPASS C5000]
SCANNERID=WorkCentre 400c Series
ADF=SHEET
REGADF=CENTER
BUFFERSIZE=PREFERRED
TWAINUI=HIDE
<END>

[Olivetti STUDIO JET 300(32 bit)]
[Xerox WorkCentre Xi]
ADF=NO
RESRANGE=100,300,100
DFLTBRIGHT=USE MSG_SET
DFLTCONTRAST=USE MSG_SET
TWOPASS=DISABLED
TWAINUI=HIDE
<END>


;-------------------------------------------------------------------------------
;The below entry is provided for documentation.
;The value in brackets should reflect the name of the twain source as is in the
;Data Source ID ProductName member of the TW_IDENTITY structure.  If you want
;to specify a particular version append:<space>Rev<space>m.n
;You may want to do this if the vendor has changed behavior in later revisions
;of the same twain source
;
;If you do not know the value you need to put in brackets do the following:
;	create a file called psapideb.ini
;	put the following lines in it
;
;		[XPAGE]
;		LOG=1
;		LOGFILE=xpage32.log
;		FLAGS1=0x80
;
;	make sure this file is in the same directory as the xscan32.psp (and this file)
;	run any product that uses xscan32.psp for scanning and use it to connect to your scanner
;	This will generate a xpage32.log file in the same directory.
;	Look for a line in xpage32.log that reads:
;	Looking up hints for Dummy Entry Rev 1.1
;	This then becomes the bracketed value that identifies the Data Source as shown below
	

[Dummy Entry Rev 1.1]

;IMPROPER CAPABILITY NEGOTIATION
;This section pertains to hinting sources that don't properly report the scanners
;capabilities.  Brightness, Contrast, Resolution and Physical Dimensions respectively.

BRIGHTRANGE=<dark value,light value,default> example:
BRIGHTRANGE=-1000,1000,0

;Set the brightness setting to its default value.  This prevents the value
;getting set to something the generates an error because of an improper value
;Some mustek scanners that don't handle brightness negotiation properly need this 
;hint
DFLTBRIGHT=USE MSG_SET

;Set brightness default value
DFLTBRIGHTVAL=100

CONTRASTRANGE=<low value,high value,default> example:
CONTRASTRANGE=-128,128,0

;Set the contrast setting to its default value.  
DFLTCONTRAST=USE MSG_SET

;Set contrast default value
DFLTCONTRASTVAL=100

RESRANGE=<min,max,step> example:
RESRANGE=75,600,50

MAXHEIGHT=<Physical Heigth of the platen in inches> example:
MAXHEIGHT=11

MAXWIDTH=<Physical Width of the platen in inches>  example:
MAXWIDTH=8.5

;SHEET FEEDER AND ADF HINTS
;The following entries can be tried to allow proper operation of scanners that do not properly
;report whether an optional ADF is attatched of if the scanner is a sheet fed only scanner
ADF=NO
ADF=YES
ADF=SHEET

;The following three entries force xscan to attempt to set and test whether there 
;is an ADF in a variety of manners for Data Sources that don't respond well
;to the conventional ways of querying the existence of an ADF.
ADF=SET
ADF=SETADF
ADF=SET&TEST

;Include the following if the scanner is a hand held scanner
ADF=HAND

;Include the proper entry below if any of binary, grey, or color scans seem inverted
INVERTB=YES
INVERTG=YES
INVERTC=YES

;TWAIN USER INTERFACE HINTS
;The following hints force the scan to take place using the Data Source's User Interface up,
;suppressed, and up only for the first scan of a multiple image scan respectively.
;The scan will proceed with the Source UI suppressed if no hint is found.  
TWAINUI=SHOW
TWAINUI=HIDE
TWAINUI=ONCE

;Include the following to disable two-pass scanning.
TWOPASS=DISABLED

;Include the following hint to force the application to allocate a buffer identical in 
;size to that used by the Data Source.  This will sometimes solve problems in which differing
;sized buffers cause the aquisition process to get out sync and data to be lost.
BUFFERSIZE=PREFERRED

;Include the below if the twain source allows setting CAP_INDICATORS off but really
;needs them to be on to work properly
INDICATORS=ON

;Include the below if the origin of the scanner is in the middle of platen.  This is common
;in Sheetfed scanners in which the paper guide slides to the center for business cards etc.
;The following corresponds to sheetfed/ADF and flatbeds respectively
REGADF=CENTER
REGFLAT=CENTER

;Include the below if the twain source only supports the native mode image transfer mechanism
;only do this if absolutely necessary as it will usually be slower and use more memory.
XFERMECH=NATIVE

;Include the below if scanner shuts off communication with application as it brings the lamp
;back to its home position. This will force xscan to sit idle for the specified amount of time
;allowing the lamp to return home before it attempts to resume communication.
ENDDELAY=<time in seconds> example:
ENDDELAY=15

;Include the below if the scanner automatically determines page size by using a black background or
;sensors on movable paper guide(s)
PAGESIZE=AUTOMATIC

;Include the below if the twain source supports ICAP_GAMMA and the default value for the twain source
;is not appropriate (please refer to the TWAIN specification)
GAMMA=<some float value, i.e. 2.2>

;Include the line below if the twain source's user interface or progress indicator comes up behind the
;scantool's user interface. 
UI=BEHIND

;Include the line below if you want to see what Capabilities the twain source says it supports.
;The decimal values of the supported caps will be listed in the log file.
;Note that this does not necessarily mean that it actually supports it.
;i.e. the DeskScan issue with AutoBrightness returning an exception only in the debugger. 
GETSUPPORTEDCAPS=YES

;Include the line below if canceling from a button in the applications user interface causes crashes
;or hangs.  This should not be used with TWAINUI=SHOW
IGNORECANCEL=YES

;Include the line below if you want to set the color bitdepth to 24 instead of the current 8.
COLORBITDEPTH24=YES

;The following hints shouldn't be used without testing in a debugging environment.  They are to overcome a 
;thread/process priority issue.  In some instances you will have multiple threads/processes running where two or more
; will receive almost all the processing time leaving one or more other threads getting hardly any.  These hints lower
; the thread priority of the calling thread before making TWAIN calls and then restore it afterwords.  The hints are 
; specific to OS since they handle setting priorities differently.

W9XPRIORITY=LOW
WNTPRIORITY=LOW
W2KPRIORITY=LOW

<END>
